
   If you are using a Sound Blaster compatible sound card and are not hearing 
   digitized speech or sounds, make sure your AUTOEXEC.BAT file contains the 
   following line...

	SET BLASTER=A220 I7 D1 T1

   ...where A### is the address of your card (220 or 240),
   I# is the interrupt (5, 7, 10), D# is the DMA 
   channel (1 or 3), and always T1.

   Please consult your sound card manual with any options regarding emulation
   of the Sound Blaster. Make sure to reboot your computer after making any 
   changes to AUTOEXEC.BAT, so that this setting will take effect.

   Also, if you have run MEMMAKER from DOS 6.2, a HIGHSCAN option may have
   been added to the EMM386 command line in your CONFIG.SYS file. If you
   experience problems, you should try removing the HIGHSCAN option.

   If you are still experiencing problems, call Virgin Technical Support at 
   714-833-1999 (USA), Paris 48-42-07-39 (France), 0-81-964-9361 (UK), 
   or 44-81-964-9361 (outside the UK).
